Order Form - Gearboxes	MA - OE - 09 - 0001
Customer

Purchase Order #

Quote #

Project / Engineer:

Page	of

Quantity:

Gearbox Type:	GS	GF

GK - :	GST :

Machining Data:

with bore and key

Diameter	:

Keyway	:

Overkey	:

special:

Style:

Degree of Travel:

Service:	STD	AWWA	BURIED	SUBMERSIBLE

Valve Mounting Flange:	Special :

Coupling (GS/GST):	BLANK	MACHINED (see right)

Output drive (GK)	:	Other:

Enclosure (NEMA):

Note Standard Enclosure Ratings listed below:

GK10.2 to GK40.2 : NEMA 4X/6

GS50.3 to GS125.3: NEMA 4X/6

G160.3 to GS500 : NEMA 4/6 *

*to meet Nema 4X, choose Stainless Steel Ext’l Fastener option. (See AUMA Sales manual for further details.)

Temperature:

Input:	Standard Input Shaft

Stainless Steel Input Shaft (where offered)**

Options:	Hand wheel (Diameter: inches)

Chain wheel (Diameter: inches) Chain: ( ft)

2” Square Nut

Standard steel ext’l fasteners (GS160 to 500)**

Other

“SA” mounting flange :	NO	YES (For use with: )

Mounted To: ( ) (Page of )

**These options affect price and delivery.

Notes:

Prepared by :	Date:	Issue 1.07

AUMA Actuators, Inc. USA

GEARBOXES

Gearboxes

Controlled ISO Document

barbarac

2007-10-02

AUMA ACTUATORS, INCORPORATED